MPEG-Surround:

MPEG >>> backward compatible

Based on SAC principle : In the encoder a mono or stereophonic downmix is generated from the multichannel inpıt signal and additional parametric side information is extracted to guide the subsequent up-mix prosedüre in the decoder.

Henders Clustering Scheme

Fixed clusters corresponding to a non uniform spatial subdıvısıon